# X-VLA: The First Soft-Prompted Robot Foundation Model for Any Robot, Any Task

## Overview

For years, robotics has aspired to build agents that can follow natural human instructions and operate dexterously across many environments and robot bodies. Recent breakthroughs in LLMs and VLMs suggest a path forward: extend these foundation-model architectures to embodied control by grounding them in actions. This has led to the rise of Vision-Language-Action (VLA) models, with the hope that a single generalist model could combine broad semantic understanding with robust manipulation skills.

But training such models is difficult. Robot data is fragmented across platforms, sensors, embodiments, and collection protocols. Heterogeneity appears everywhere: different arm configurations, different action spaces, different camera setups, different visual domains, and different task distributions. These inconsistencies create major distribution shifts that make pretraining unstable and adaptation unreliable.

Inspired by meta-learning and prompt learning, we ask: **"What if a VLA model could learn the structure of each robot and dataset the same way LLMs learn tasks, through prompts?"**

**X-VLA** is a soft-prompted, flow-matching VLA framework that treats each hardware setup as a "task" and encodes it using a small set of learnable embeddings. These **Soft Prompts** capture embodiment and domain-specific variations, guiding the Transformer from the earliest stages of multimodal fusion. With this mechanism, X-VLA can reconcile diverse robot morphologies, data types, and sensor setups within a single unified architecture.

  

Built from pure Transformer encoders, X-VLA scales naturally with model size and dataset diversity. Across 6 simulation benchmarks and 3 real robots, Soft Prompts consistently outperform existing methods in handling hardware and domain differences. X-VLA-0.9B, trained on 290K episodes spanning seven robotic platforms, learns an embodiment-agnostic generalist policy in Phase I, and adapts efficiently to new robots in Phase II simply by learning a new set of prompts, while keeping the backbone frozen.

  

With only 1% of parameters tuned (9M), X-VLA-0.9B achieves near-π₀ performance on LIBERO and Simpler-WidowX, despite using **300× fewer trainable parameters**. It also demonstrates strong real-world dexterity with minimal demonstrations, including folding cloths in under two minutes.

  

X-VLA shows that generalist robot intelligence does not require increasingly complex architectures, only the right way to absorb heterogeneity. Soft Prompts offer a simple, scalable mechanism for unifying diverse robotic data, paving the way toward adaptable, cross-embodiment robot foundation models.

## Installation

After installing LeRobot, install the X-VLA dependencies:

```bash
pip install -e .[xvla]
```

After the new release, you'll be able to do:

```bash
pip install lerobot[xvla]
```

## Quick Start

### Basic Usage

To use X-VLA in your LeRobot configuration, specify the policy type as:

```bash
policy.type=xvla
```

### Evaluating Pre-trained Checkpoints

Example evaluation with LIBERO:

```bash
lerobot-eval \
  --policy.path="lerobot/xvla-libero" \
  --env.type=libero \
  --env.task=libero_spatial,libero_goal,libero_10 \
  --env.control_mode=absolute \
  --eval.batch_size=1 \
  --eval.n_episodes=1 \
  --env.episode_length=800 \
  --seed=142
```

## Available Checkpoints

### 🎯 Base Model

**[lerobot/xvla-base](https://huggingface.co/lerobot/xvla-base)**

A 0.9B parameter instantiation of X-VLA, trained with a carefully designed data processing and learning recipe. The training pipeline consists of two phases:

- **Phase I: Pretraining** - Pretrained on 290K episodes from Droid, Robomind, and Agibot, spanning seven platforms across five types of robotic arms (single-arm to bi-manual setups). By leveraging soft prompts to absorb embodiment-specific variations, the model learns an embodiment-agnostic generalist policy.

- **Phase II: Domain Adaptation** - Adapted to deployable policies for target domains. A new set of soft prompts is introduced and optimized to encode the hardware configuration of the novel domain, while the pretrained backbone remains frozen.

### Simulation Checkpoints

**[lerobot/xvla-libero](https://huggingface.co/lerobot/xvla-libero)**

Achieves 93% success rate on LIBERO benchmarks. Fine-tuned from the base model for simulation tasks.

**[lerobot/xvla-widowx](https://huggingface.co/lerobot/xvla-widowx)**

Fine-tuned on BridgeData for pick-and-place experiments on compact WidowX platforms. Demonstrates robust manipulation capabilities.

### 🤖 Real-World Checkpoints

**[lerobot/xvla-folding](https://huggingface.co/lerobot/xvla-folding)**

A fine-tuned dexterous manipulation model trained on the high-quality Soft-FOLD cloth folding dataset. Achieves 100% success rate over 2 hours of continuous cloth folding.

**[lerobot/xvla-agibot-world](https://huggingface.co/lerobot/xvla-agibot-world)**

Optimized for AgileX robot dexterous manipulation tasks.

**[lerobot/xvla-google-robot](https://huggingface.co/lerobot/xvla-google-robot)**

Adapted for Google Robot platforms.

## Training X-VLA

### Recommended Training Configuration

When fine-tuning X-VLA for a new embodiment or task, we recommend not freezing the VLM, and also setting the `policy.dtype=bfloat16` to not hit OOM errors.

```bash
lerobot-train \
  --dataset.repo_id=YOUR_DATASET \
  --output_dir=./outputs/xvla_training \
  --job_name=xvla_training \
  --policy.path="lerobot/xvla-base" \
  --policy.repo_id="HF_USER/xvla-your-robot" \
  --policy.dtype=bfloat16 \
  --policy.action_mode=auto \
  --steps=20000 \
  --policy.device=cuda \
  --policy.freeze_vision_encoder=false \
  --policy.freeze_language_encoder=false \
  --policy.train_policy_transformer=true \
  --policy.train_soft_prompts=true \
```

### Training Parameters Explained

| Parameter                  | Default | Description                                    |
| -------------------------- | ------- | ---------------------------------------------- |
| `freeze_vision_encoder`    | `false` | Do not freeze the VLM vision encoder weights   |
| `freeze_language_encoder`  | `false` | Do not freeze the VLM language encoder weights |
| `train_policy_transformer` | `true`  | Allow policy transformer layers to train       |
| `train_soft_prompts`       | `true`  | Allow soft prompts to train                    |

**💡 Best Practice**: For Phase II adaptation to new embodiments, do not freeze the VLM encoders and also train the policy transformer and soft prompts.

### Example: Training on Bimanual Robot

```bash
lerobot-train \
  --dataset.repo_id=/bimanual-so100-handover-cube \
  --output_dir=./outputs/xvla_bimanual \
  --job_name=xvla_so101_training \
  --policy.path="lerobot/xvla-base" \
  --policy.dtype=bfloat16 \
  --policy.repo_id="YOUR_USERNAME/xvla-biso101" \
  --steps=3000 \
  --policy.device=cuda \
  --policy.action_mode=so101_bimanual \
  --policy.freeze_vision_encoder=false \
  --policy.freeze_language_encoder=false \
  --policy.train_policy_transformer=true \
  --policy.train_soft_prompts=true
```

💡 **Best Performance:** If you have sufficient computational resources and want to achieve best X-VLA finetuning performance, you should follow the official finetuning strategy:

**🔥 Full-finetune all components with a custom learning-rate scheme**

To ensure stable optimization, the Vision-Language Model (VLM) must be trained with only 1/10 of the base learning rate, while all other components use the full LR.
This LR ratio is crucial for achieving strong and stable finetuning performance. This is already done for you by default.
❕Note

Completely matching the official reported performance may require an additional warm-up LR schedule for soft-prompts, which can bring minor improvements.
We encourage implementing this in your customized training pipeline for optimal results.

## Core Concepts

### 1. Action Modes

X-VLA uses an **Action Registry** system to handle different action spaces and embodiments. The `action_mode` parameter defines how actions are processed, what loss functions are used, and how predictions are post-processed.

#### Available Action Modes

| Action Mode      | Action Dim              | Description                                 | Use Case                             |
| ---------------- | ----------------------- | ------------------------------------------- | ------------------------------------ |
| `ee6d`           | 20                      | End-effector with xyz, 6D rotation, gripper | Dual-arm setups with spatial control |
| `joint`          | 14                      | Joint-space with gripper                    | Direct joint control robots          |
| `agibot_ee6d`    | 20                      | AGI-bot variant with MSE loss               | AGI-bot platforms                    |
| `so101_bimanual` | 20 (model), 12 (real)   | SO101 bimanual robot                        | Bimanual manipulation tasks          |
| `auto`           | 20 (model), auto (real) | Auto-detects action dim from dataset        | **Recommended** for new robots       |

#### Why Action Modes Matter

When you have a pretrained checkpoint like `lerobot/xvla-base` trained with `action_dim=20`, and you want to train on a dataset with a different action dimension (e.g., 14 for bimanual arms), you can't simply trim the action dimension. The action mode orchestrates:

1. **Loss Computation**: Different loss functions for different action components (MSE for joints, BCE for grippers, etc.)
2. **Preprocessing**: Zeroing out gripper channels, padding dimensions
3. **Postprocessing**: Applying sigmoid to gripper logits, trimming padding

#### Example: BimanualSO101 Action Space

The `so101_bimanual` action mode handles the mismatch between model output (20D) and real robot control (12D):

```python
# Model outputs 20 dimensions for compatibility
dim_action = 20

# Real robot only needs 12 dimensions
# [left_arm (6), right_arm (6)] = [joints (5) + gripper (1)] × 2
REAL_DIM = 12

# Preprocessing: Pad 12D actions to 20D for training
# Postprocessing: Trim 20D predictions to 12D for deployment
```

See the [action_hub.py](/home/jade_choghari/robot/lerobot/src/lerobot/policies/xvla/action_hub.py) implementation for details.

#### Auto Action Mode (Recommended)

The `auto` action mode is the easiest way to use X-VLA with any robot. It automatically detects your dataset's action dimension and handles padding/trimming:

```bash
lerobot-train \
  --policy.path="lerobot/xvla-base" \
  --policy.action_mode=auto \
  --policy.max_action_dim=20 \
  ...
```

**How it works:**

- Reads `action_feature.shape[-1]` from your dataset (e.g., 7 for Franka)
- Model outputs `max_action_dim` (default 20) for pretrained compatibility
- Loss is computed **only on the real dimensions**: `MSE(pred[:,:,:real_dim], target[:,:,:real_dim])`
- Postprocess trims output back to `real_dim` for robot control

This eliminates the need to create custom action modes for most robots.

### 2. Domain IDs

Domain IDs are learnable identifiers for different robot configurations and camera setups. They allow X-VLA to distinguish between:

- Different robots (Robot 1 vs Robot 2)
- Different camera configurations (cam1 vs cam2)
- Different combinations (Robot1-cam1-cam2 vs Robot1-cam1 vs Robot2-cam1)

#### Setting Domain IDs

**During Training**: By default, domain_id is set to 0 for general training.

**During Evaluation**: Specify the domain_id that matches your checkpoint's training configuration.

```python
# Example: LIBERO checkpoint uses domain_id=3
domain_id = 3
```

The domain_id is automatically added to observations by the `XVLAAddDomainIdProcessorStep` in the preprocessing pipeline.

The `lerobot/xvla-base` model has been trained on the following domain IDs. It is recommended to choose one that most resembles your robot/configuration:

#### Fine-tuning Datasets

| Dataset Name     | Domain ID |
| ---------------- | --------- |
| Bridge           | 0         |
| RT1              | 1         |
| Calvin           | 2         |
| libero           | 3         |
| widowx-air       | 4         |
| AIR-AGILEX-HQ    | 5         |
| robotwin2_abs_ee | 6         |
| robotwin2_clean  | 6         |
| robocasa-human   | 7         |
| VLABench         | 8         |
| AGIBOT-challenge | 9         |
| AIR-AGILEX       | 10        |
| AIRBOT           | 18        |

### 3. Processor Steps

X-VLA requires specific preprocessing and postprocessing steps for proper operation.

#### Required Preprocessing Steps

1. **XVLAImageToFloatProcessorStep**: Converts images from [0, 255] to [0, 1] range
2. **XVLAImageNetNormalizeProcessorStep**: Applies ImageNet normalization (required for VLM backbone)
3. **XVLAAddDomainIdProcessorStep**: Adds domain_id to observations

#### Example Custom Processor

For LIBERO environments, a custom processor handles the specific observation format:

```python
from lerobot.policies.xvla.processor_xvla import LiberoProcessorStep

processor = LiberoProcessorStep()
# Handles robot_state dictionary, converts rotation matrices to 6D representation
# Applies 180° image rotation for camera convention
```

### 4. Configuration Parameters

Key configuration parameters for X-VLA:

```python
# Observation and action
n_obs_steps: int = 1          # Number of observation timesteps
chunk_size: int = 32           # Action sequence length
n_action_steps: int = 32       # Number of action steps to execute

# Model architecture
hidden_size: int = 1024        # Transformer hidden dimension
depth: int = 24                # Number of transformer layers
num_heads: int = 16            # Number of attention heads
num_domains: int = 30          # Maximum number of domain IDs
len_soft_prompts: int = 32     # Length of soft prompt embeddings

# Action space
action_mode: str = "ee6d"      # Action space type (use "auto" for auto-detection)
use_proprio: bool = True       # Use proprioceptive state
max_state_dim: int = 32        # Maximum state dimension
max_action_dim: int = 20       # Max action dim for padding (used by "auto" mode)

# Vision
num_image_views: int | None    # Number of camera views
resize_imgs_with_padding: tuple[int, int] | None  # Target image size with padding

# Training
num_denoising_steps: int = 10  # Flow matching denoising steps
```

## Creating Custom Action Modes

If your robot has a unique action space, you can create a custom action mode:

### Step 1: Define Your Action Space

```python
from lerobot.policies.xvla.action_hub import BaseActionSpace, register_action
import torch.nn as nn

@register_action("my_custom_robot")
class MyCustomActionSpace(BaseActionSpace):
    """Custom action space for my robot."""

    dim_action = 15  # Your robot's action dimension
    gripper_idx = (7, 14)  # Gripper channel indices

    def __init__(self):
        super().__init__()
        self.mse = nn.MSELoss()
        self.bce = nn.BCEWithLogitsLoss()

    def compute_loss(self, pred, target):
        """Define your loss computation."""
        # Example: MSE for joints, BCE for grippers
        joints_loss = self.mse(pred[:, :, :7], target[:, :, :7])
        gripper_loss = self.bce(pred[:, :, self.gripper_idx],
                                target[:, :, self.gripper_idx])

        return {
            "joints_loss": joints_loss,
            "gripper_loss": gripper_loss,
        }

    def preprocess(self, proprio, action, mode="train"):
        """Preprocess actions before training."""
        # Example: Zero out grippers in proprioception
        proprio_m = proprio.clone()
        action_m = action.clone() if action is not None else None
        proprio_m[..., self.gripper_idx] = 0.0
        if action_m is not None:
            action_m[..., self.gripper_idx] = 0.0
        return proprio_m, action_m

    def postprocess(self, action):
        """Post-process predictions for deployment."""
        # Example: Apply sigmoid to gripper logits
        action[..., self.gripper_idx] = torch.sigmoid(action[..., self.gripper_idx])
        return action
```

### Step 2: Use Your Custom Action Mode

```bash
lerobot-train \
  --policy.action_mode=my_custom_robot \
  --dataset.repo_id=YOUR_DATASET \
  --policy.path="lerobot/xvla-base" \
  ...
```

## Advanced Topics

### Multi-Camera Support

X-VLA supports multiple camera views through the `num_image_views` parameter:

```python
# Configure for 3 camera views
policy.num_image_views=3

# Add empty cameras if you have fewer physical cameras
policy.empty_cameras=1  # Adds 1 zero-padded camera view
```

### Custom Preprocessing Pipeline

Create a custom preprocessing pipeline for your environment:

```python
from lerobot.processor import PolicyProcessorPipeline
from lerobot.policies.xvla import (
    XVLAImageToFloatProcessorStep,
    XVLAImageNetNormalizeProcessorStep,
    XVLAAddDomainIdProcessorStep,
)

# Build custom pipeline
preprocessor = PolicyProcessorPipeline(
    steps=[
        YourCustomProcessorStep(),  # Your custom processing
        XVLAImageToFloatProcessorStep(),  # Required: convert to float
        XVLAImageNetNormalizeProcessorStep(),  # Required: ImageNet norm
        XVLAAddDomainIdProcessorStep(domain_id=5),  # Your domain ID
    ]
)
```

### Handling Different Action Dimensions

When your dataset has fewer action dimensions than the pretrained model:

**Option 1 (Recommended)**: Use `auto` action mode

```bash
# Automatically detects your dataset's action dimension
# Works with any robot without custom code
policy.action_mode=auto
policy.max_action_dim=20  # Match pretrained model
```

**Option 2**: Use a predefined action mode with built-in padding

```python
# Model expects 20D, dataset has 12D
# Action mode handles padding internally
action_mode = "so101_bimanual"  # Pads 12 → 20
```

**Option 2**: Create a custom action mode that maps dimensions explicitly

```python
@register_action("my_mapped_action")
class MappedActionSpace(BaseActionSpace):
    dim_action = 20
    REAL_DIM = 12

    def _pad_to_model_dim(self, x):
        # Custom padding logic
        ...
```

## Troubleshooting

### Common Issues

**Issue**: "Action dimension mismatch"

- **Solution**: Check that your `action_mode` matches your robot's action space. Create a custom action mode if needed.

**Issue**: "Image values outside [0, 1] range"

- **Solution**: Ensure images are preprocessed with `XVLAImageToFloatProcessorStep` before normalization.

**Issue**: "Domain ID not found"

- **Solution**: Make sure `XVLAAddDomainIdProcessorStep` is in your preprocessing pipeline with the correct domain_id.

**Issue**: "Low success rate on new embodiment"

- **Solution**:
  1. Verify your action_mode is correct
  2. Check that soft prompts are being trained (`train_soft_prompts=True`)
  3. Ensure proper preprocessing (ImageNet normalization, domain_id)
  4. Consider increasing training steps

**Issue**: "Out of memory during training"

- **Solution**:
  1. Reduce `chunk_size` (e.g., from 32 to 16)
  2. Enable gradient checkpointing
  3. Reduce batch size
  4. Freeze more components

## Citation

If you use X-VLA in your research, please cite:

```bibtex
@article{zheng2025x,
  title   = {X-VLA: Soft-Prompted Transformer as Scalable Cross-Embodiment Vision-Language-Action Model},
  author  = {Zheng, Jinliang and Li, Jianxiong and Wang, Zhihao and Liu, Dongxiu and Kang, Xirui
             and Feng, Yuchun and Zheng, Yinan and Zou, Jiayin and Chen, Yilun and Zeng, Jia and others},
  journal = {arXiv preprint arXiv:2510.10274},
  year    = {2025}
}
```

## Additional Resources

- [X-VLA Paper](https://arxiv.org/pdf/2510.10274)
- [LeRobot Documentation](https://github.com/huggingface/lerobot)
- [Action Registry Implementation](https://github.com/huggingface/lerobot/src/lerobot/policies/xvla/action_hub.py)
- [Processor Implementation](https://github.com/huggingface/lerobot/src/lerobot/policies/xvla/processor_xvla.py)
- [Model Configuration](https://github.com/huggingface/lerobot/src/lerobot/policies/xvla/configuration_xvla.py)

## Contributing

We welcome contributions! If you've implemented a new action mode or processor for your robot, please consider submitting a PR to help the community.

